BLE:

* Advertising: 0.90 mA
* Transmitting at 128 kbps:
  + 40 uS ramp up: 6.85 mA
  + Steady-state: 6.0 mA