Meeting: Undergraduates + GW

Location OEDK 104

Battery:

* P13: doesn’t work
  + Less than 3.0 V
* Alternatives:
  + Larger pr44 that has enough voltage is too big (the battery holder) to fit on board with the jumpers
    - Could make custom battery holder
    - Or smush parts together
  + Smaller silver oxide does fit and has enough voltage, but we would have less capacity (only 60 mAh)
  + We could do all alternatives and hope that we can make pr44 custom holder, else we use the silver oxide
* Nordics out of stock :(:(:(:(
  + Order older revisions that should work with the software stack
* Revisions and finalize pcb
  + Trim back spacing between nordic chip and pins on pcb so that the spacing is not as tight

Nordic:

* Should try to get event handler to do compression and reading at the same time.
* May take a while
* Need to add in ble with everything else as well.